1. CHC EasyNav has several useful features. Of the following which one is a feature.
a. Ability to Import a design
b. Load point data collected with a rover
c. Upgradable system
2. The system has two antennas installed on the boom of the machine. Which antenna is considered the main antenna?
a. Front
b. Back
3. The system has two GNSS antenna connection ports on the back of the display. Which antenna port is for the Aux Antenna.

4. The bucket sensor can be installed on which of the following (Choose all that apply)
a. Bucket
b. Dog bone
c. Quick Coupler
d. Bucket Linkage
5. When pulling measurements for the GNSS antennas. The measurement should be based on where on the antenna?
a. The reference mark on the bracket
b. Back of bracket
c. Outside edge of antenna
6. A framing square is needed for the calibration. Which routine is the square used for?
a. Measuring the boom thickness
b. Used to measure the stick length
c. Utilized for the O-M and O-P for the stick pin
7. When conducting training what is the first thing you should show a customer?
a. How to create a surface design
b. Connecting to a radio
c. How to change buckets
d. Screen Layout (User Interface)
8. What is the remote support application on the system called?
a. Mobi Control
b. Quick Support
c. SiteLink
d. Google Chrome
9. Will the EasyNav system work on a swing boom machine without additional hardware?
a. True
b. False
10. The recommended install and calibration time is?
a. 8 Hours
b. 16 Hours
c. 4 Hours
d. None of the above

11. The kit provides weld on brackets. Where is the proper location to weld while installing the weld on brackets?
a. Top and bottom of bracket
b. Left and Right Side of the bracket
c. Center holes on bracket
d. All the above
12. When determining the location for the display it is important to check for the following? 
a. Front glass clearance
b. Operators view from seat
c. OEM gauge clearance
d. All of the above
13. When installing the main GNSS antenna it is best to install the bracket?
a. Within 1 m of the stick pin towards the bottom of the boom
b. Within 1 m of the stick pin towards the top of the boom
c. On the stick pin
d. None of the above
14. After calibration a flat to vertical bucket check is performed. What does this check confirm?
a. The bucket is calibrated correctly
b. The Stick is properly calibrated
c. All hardware is installed properly
d. None of the above
15. The system can not be calibrated on the following unit of measurements?
a. US Survey Feet 0.01’
b. Meters
c. Feet and Inches 
16. When calibrating the bucket sensor, if the sensor is installed on the quick coupler. The tech must ensure the dog bone is horizontal before calibrating?
a. True
b. False
17. All measurements based on the pins are measured to the_____ of the pin?
18. What are the two types of power connection available for the system?
19. All the sensors including the GNSS antennas must be installed on the same side of the boom?
a. True
b. False
20. When align the sensor before welding they should be______ to the centerline of the pins?
a. Parallel
b. Perpendicular
c. Does not matter


21. While installing the GNSS antennas it is important for the connection port to be facing in which direction?
a. Connector towards machine cab
b. Connector towards bucket
c. Connector towards boom facing inwards
22. Each sensor has an arrow indicating the direction the sensor should be installed. Which is the correct orientation of the arrow
a. Towards the Cab
b. Facing upperwards
c. Facing downwards
d. Towards the bucket
23. What are the two connection types that give you a fixed position in the system?
a. Radio and Surface
b. Surface and Network(CORS)
c. Radio and Network(CORS)
24. There is more than one way to view recorded points within the system
a. True
b. False
25. What is the purpose of the bucket focus point button?
a. It shows the size of the bucket
b. It shows which bucket tooth will read grade
c. It changes coordinate systems
d. All of the above
26. You can not edit a surface after you have created it
a. True 
b. False 
27. You can create a surface from both the bucket teeth or a recorded point?
a. True
b. False
28. The purpose of the Coordinate system is?
a. Place a machine within a certain state boundary
b. Change buckets 
c. Broadcast a frequency 
d. None of the above
29. When setting up a radio connection for the machine what settings icon is it located within?
a. System
b. Datalink
c. About
d. Point management

Please email the completed test to remoteInstall@benchmarksupply.com, please include your contact information in the email body and with your availability to follow up with Benchmark to discuss before proceeding with installation.
